DIST500-Configuration 3.8.2.173-TP

  DIST500-Configuration.exe
  DIST500-Configuration.exe [-com#] [-sendaddr=#] [-ipaddr=#.#.#.#] [-sensorurl]

  -com#             Load serial port
        #           Port number, e.g. -com1
                    Loads driver for serial port.
    
  -sendaddr=#       Sender's UIP address
        #           UIP adress from 240 through 254 e.g. -sendaddr=250
                    Assigns tool's UIP address. Default is 252.

  -ipaddr=#.#.#.#   States IP address of the PC.
        #.#.#.#     IP address, e.g. -ipaddr=172.30.31.10
                    Binds tool to an IP address of the PC where communication shall happen. 
                    Setting is necessary when more than one network interface is present.

  -sensorurl        Communicate with sensor(s) via their URL(s)
                    One or more sensors may be communicated to directly via their URLs, e.g.
                    udp://10.3.1.128#1 
                    This allows access across routers. 
                    This configuration skips the sensor selection dialog.
