2017-05-29 Unreleased prototype version 3.8.2.173-TP
====================================================
Feature:
- Parameter Version changed to 1.4.
- Additional installation parameters for new counter adjustable

2017-01-27 Release 3.8.2.172
================================
Feature:
- Improved (reduced) memory usage

Bugfix:
- Removed exception during container update combined with sensors that change their IP addresses (DHCP).

2017-01-27 Release 3.8.1.171
================================
Feature:
- Firmware container (.d5fc) update can now handle sensors restarting with
  dynamic IP addresses (DHCP).
- Configuration readout is more fault-tolerant.

Bugfix:
- Fixed some error message wordings.

2016-10-10 Bugfix Release 3.8.0.169
================================
Bugfix:
- Further D5FC update improvement to ensure repeatability

Feature:
- New message with instructions for how to handle
  a special error case in container updates

2016-10-06 Bugfix Release 3.7.3.168
================================
Bugfix:
- D5FC update improved to ensure repeatability

Bugfix:
- Count Category Ids are configured incorrectly by Build Group, Change Group and Ungroup.

Feature:
- SNTP-Server Addresses are shown

2016-07-12 Bugfix Release 3.7.1.165
================================
Bugfix:
- Build Group, Change Group and Ungroup does not allow zero Gateway address.

2016-07-12 Bugfix Release 3.7.0.164
================================
Feature:
- Tool can now read and write new ComponentGroup parameters productionIndex and productionId

Bugfix:
- Image files are still opened after flashing
- Changed filter size units to "px" instead of "mm".

2016-06-10 Bugfix Release 3.6.1.163
================================
Bugfix:
- command line parameter -ipaddr=xxx.xxx.xxx.xxx was not passed to sensor choice dialogue

2016-05-27 Bugfix Release 3.6.1.162
================================
Bugfix:
- Door Clear parameter are always displayed.

2016-04-29 Feature Release 3.6.0.161
================================
Features:
- Driver options are now configurable from the graphical interface
- New IP scan interface for networks where sensor discovery via broadcast is blocked by routers
Usability:
- Plausability check for driver options bars the user from setting obviously wrong options
- Driver options are saved to and loaded from a file in the user's directory
- Number of detected sensors is displayed

