 Error codes - DIST500-Configuration in mode for automatic updates
====================================================================

0x0000: OK              // RESULT_SUCCESS
0x0001: Error           // RESULT_FAILED

0x0002: Wrong parameter of wrong number of paramters   // WRONG_PARAMETER
0x0003: Error opening sensor list file                 // OPEN_FILE_LIST_FAILED
0x0004: Error opening default drivers                  // LOAD_DEFAULT_DRIVER_FAILED
0x0005: Log file could not be opened                   // CANNOT_OPEN_LOG_FILE
0x0006: Wrong sensor URL                               // WRONG_SENSOR_URL
0x0007: Sensor was not found                           // SENSOR_NOT_FOUND
0x0008: Error reading container file                   // READ_CONTAINER_FILE_FAILED

0x0100: Error on setting a work-mode                     // SET_WORKING_MODE_FAILED
0x0101: Query of sensor information failed               // GET_SENSOR_INFO_FAILED
0x0102: Loading of configuratin data from Flash failed   // RESTORE_CONFIG_FAILED
0x0103: Reading of configuration data failed             // READ_CONFIG_FAILED
0x0104: Query of sensor status failed                    // GET_SENSOR_STATUS_FAILED
0x0105: Restart failed                                   // RESTART_FAILED

0x0200: Update via container file -
        Error setting work-mode after firmware update      // CONTAINER_SET_WORKING_MODE_AFTER_UPDATE_FAILED
0x0201: Update via container file -
        Update of application firmware failed              // CONTAINER_APPLICATION_UPDATE_FAILED
0x0202: Update via container file -
        Verification of application firmware failed        // CONTAINER_APPLICATION_VERIFY_FAILED
0x0203: Update via container file -
        Update of communication firmware failed            // CONTAINER_COMMUNICATION_UPDATE_FAILED
0x0204: Update via container file -
        Verification of communication firmware failed      // CONTAINER_COMMUNICATION_VERIFY_FAILED
0x0205: Update via container file -
        Update of first FPGA image failed                  // CONTAINER_FIRST_FPGA_UPDATE_FAILED
0x0206: Update via container file -
        Verification of first FPBA image failed            // CONTAINER_FIRST_FPGA_VERIFY_FAILED
0x0207: Update via container file -
        Update of second FPGA image failed                 // CONTAINER_SECOND_FPGA_UPDATE_FAILED
0x0208: Update via container file -
        Verification of second FPGA image failed           // CONTAINER_SECOND_FPGA_VERIFY_FAILED
0x0209: Update via container file -
        Reading of configuration data failed               // CONTAINER_READ_CONFIGURATION_FAILED
0x020A: Update via container file -
        Writing of configuration data failed               // CONTAINER_WRITE_CONFIGURATION_FAILED
0x020B: Update via container file -
        Writing of configuration data to flash failed      // CONTAINER_SAVE_CONFIGURATION_FAILED
0x020C: Update via container file -
        Writing of mismatch parameters failed              // CONTAINER_SAVE_MISMATCH_CONFIGURATION_FAILED

0x0300: Update of application firmware failed          // APPLICATION_UPDATE_FAILED
0x0301: Verification of application firmware failed    // APPLICATION_VERIFY_FAILED
0x0302: Update of communication firmware failed        // COMMUNICATION_UPDATE_FAILED
0x0303: verification of communication firmware failed  // COMMUNICATION_VERIFY_FAILED
0x0304: Update of first FPGA image failed              // FIRST_FPGA_UPDATE_FAILED
0x0305: Verification of first FPGA image failed        // FIRST_FPGA_VERIFY_FAILED
0x0306: Update of second FPGA image failed             // SECOND_FPGA_UPDATE_FAILED
0x0307: Verification of second FPGA image failed       // SECOND_FPGA_VERIFY_FAILED

